

 **Technical specifications, quality and conditions for the quotation required**

 **Steel Sheet Pile**

****

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Width | Height | Thicknesst | Sectional area | Weight per pile | Weight per wall | Moment of Inertia | Modulus of Section |
| w | h |
| mm | mm | mm | cm2/m | kg/m | kg/m2 | cm4/m | cm3/m |
| 737 | 418 | 8 | 126,4  | 73,21 | 99,3 | 35877 | 1718 |

**Specifications (Steel A 572, Grade 60, Z-shaped, which complies with the standard AASHTO M 202M or M 223M)**

***Amounts***

**2442 Parts of 11.6 meters long and 950 Parts of 13.5 meters long, (Total in tones 3012.75 TON)**

***Destination Port***

Please quote to Caldera

***Other applications***

Send Quality Certification (This is mandatory)